[nwsdata]
version="3.1.032"
autoexec_anchor="net start"
config_anchor="workgrp.sys"
default_transport=ms$netbeui

[workgroup]
descr="Workgroup Drivers"
install=delete_drivers
devdir=9:workgrp.sys
netdir=A:net.exe,9:net.msg,9:neth.msg
device=workgrp.sys,@devdir\workgrp.sys,protman.dos
sysparm=386Enh,netheapsize,20,minval
sysparm=standard,netheapsize,8,minval
lastdrive=Z

[ncd_card_specific]
243=TRANSCEIVER
301=IOCHRDY

[ncd_trans_specific]
101=MediaType

[netcard]
;   key = description, MSID, type, media, mode, install, protini, style
;       key:            unique identifier
;       description:    text description in quotes
;       MSID:           card detection id (see carddefs.h)
;       type:           ndis|ndis_sngl|mono
;       media:          arcnet|baseband|broadband|ethernet|fddi|tokenring
;       mode:           real|vxd
;       install:        section name of install script
;       protini:        section name of protocol.ini script
;       style:          0x0001  Not compatible with prot-mode protocols
;                       0x0002  Not compatible with IPX protocols
;
;
; The cards are organised in alphabetical order according to the name
; of the card.  Make sure you keep them in order if you add a new card

ms$elnk16="3Com EtherLink 16",246,ndis,ethernet,real,ms$elnk16,ms$elnk16_nif
ms$elnkii="3Com EtherLink II or IITP (8 or 16-bit)",243,ndis,ethernet,real,ms$elnkii,ms$elnkii_nif
ms$elnk3="3Com EtherLink III",247,ndis,ethernet,real,ms$elnk3,ms$elnk3_nif
ms$elnkmc="3Com EtherLink/MC",104,ndis,ethernet,real,ms$elnkmc,ms$elnkmc_nif
ms$elnkpl="3Com EtherLink Plus",241,ndis,ethernet,real,ms$elnkpl,ms$elnkpl_nif
ms$toklnk="3Com TokenLink",244,ndis,tokenring,real,ms$toklnk,ms$toklnk_nif
ms$am2100="Advanced Micro Devices AM2100/PCnet",561,ndis,ethernet,real,ms$am2100,ms$am2100_nif
ms$am210xt="Amplicard AC 210/XT",321,ndis,ethernet,real,ms$ne1000,ms$ne1000_nif
ms$am210at="Amplicard AC 210/AT",322,ndis,ethernet,real,ms$ne2000,ms$ne2000_nif
ms$arcclone="ARCNET Compatible",804,ndis,arcnet,real,ms$SMCARC,ms$genarc_nif
ms$ae1="Artisoft AE-1",311,ndis,ethernet,real,ms$ne1000,ms$ae1_nif
ms$ae2="Artisoft AE-2 or AE-3",312,ndis,ethernet,real,ms$ne2000,ms$ae2_nif
ms$ae2mca="Artisoft AE-2 (MCA) or AE-3 (MCA)",121,ndis,ethernet,real,ms$ne2000,ms$ae2mca_nif
;ms$ae3="Artisoft AE-3",313,ndis,ethernet,real,ms$ne2000,ms$ae2_nif
ms$cbl20="Cabletron E2000 Series DNI",511,ndis,ethernet,real,ms$cbl20xx,ms$cbl20xx_nif
ms$cbl21="Cabletron E2100 Series DNI",512,ndis,ethernet,real,ms$cbl21xx,ms$cbl21xx_nif
ms$dca10="DCA 10 Mb",261,ndis,ethernet,real,ms$DCA10,ms$DCA10_nif
ms$dca10fo="DCA 10 Mb Fiber Optic",262,ndis,ethernet,real,ms$DCA10,ms$DCA10_nif
ms$dca10mc="DCA 10 Mb MCA",120,ndis,ethernet,real,ms$DCA10,ms$DCA10mc_nif
ms$dca10tp="DCA 10 Mb Twisted Pair",263,ndis,ethernet,real,ms$DCA10,ms$DCA10_nif
ms$decgen="DEC Ethernet (All Types)",801,ndis,ethernet,real,ms$DEC_EW,ms$decgen_nif
ms$depca="DEC DEPCA",231,ndis,ethernet,real,ms$DEC_EW,ms$depca_nif
ms$ee101="DEC EE101 (Built-In)",238,ndis,ethernet,real,ms$DEC_EW,ms$de100_nif
ms$ewlc="DEC EtherWorks LC",232,ndis,ethernet,real,ms$DEC_EW,ms$de100_nif
ms$ewlctp="DEC EtherWorks LC/TP",234,ndis,ethernet,real,ms$DEC_EW,ms$de100_nif
ms$ewlctpb="DEC EtherWorks LC/TP_BNC",237,ndis,ethernet,real,ms$DEC_EW,ms$de100_nif
ms$ewmc="DEC EtherWorks MC",113,ndis,ethernet,real,ms$DEC_EW,ms$de210_nif
ms$ewmctp="DEC EtherWorks MC/TP",114,ndis,ethernet,real,ms$DEC_EW,ms$de210_nif
ms$ewmctpb="DEC EtherWorks MC/TP_BNC",115,ndis,ethernet,real,ms$DEC_EW,ms$de210_nif
ms$ewtrb="DEC EtherWorks Turbo",233,ndis,ethernet,real,ms$DEC_EW,ms$de200_nif
ms$ewtrbtp="DEC EtherWorks Turbo/TP",235,ndis,ethernet,real,ms$DEC_EW,ms$de200_nif
ms$ewtbtpb="DEC EtherWorks Turbo/TP_BNC",236,ndis,ethernet,real,ms$DEC_EW,ms$de200_nif
ms$decpc="DECpc 433 WS (Built-In)",239,ndis,ethernet,real,ms$DEC_EW,ms$decpc_nif
ms$spdlk16="Everex SpeedLink /PC16 (EV2027)",331,ndis,ethernet,real,ms$spdlk16,ms$spdlk16_nif
ms$hp27250="HP PC LAN Adapter/8 TL (HP27250)",343,ndis,ethernet,real,ms$HPLANB,ms$hplanb_nif
ms$hp27245="HP PC LAN Adapter/8 TP (HP27245)",341,ndis,ethernet,real,ms$HPLANB,ms$hplanb_nif
ms$hp27247A="HP PC LAN Adapter/16 TP (HP27247A)",342,ndis,ethernet,real,ms$HPLANB,ms$hplanb_nif
ms$genibmtok="IBM Token Ring (All Types)",807,ndis,tokenring,real,ms$IBMTOK,ms$genibmtok_nif
ms$ibmtr1="IBM Token Ring",201,ndis,tokenring,real,ms$IBMTOK,ms$ibmtr1_nif
ms$ibmtra="IBM Token Ring (MCA)",106,ndis,tokenring,real,ms$IBMTOK,ms$ibmtra_nif
ms$ibmtr2="IBM Token Ring II",202,ndis,tokenring,real,ms$IBMTOK,ms$ibmtr2_nif
ms$ibmtr2s="IBM Token Ring II/Short",203,ndis,tokenring,real,ms$IBMTOK,ms$ibmtr2_nif
ms$ibmtr4="IBM Token Ring 4/16Mbs",204,ndis,tokenring,real,ms$IBMTOK,ms$ibmtr4_nif
ms$ibmtr4a="IBM Token Ring 4/16Mbs (MCA)",107,ndis,tokenring,real,ms$IBMTOK,ms$ibmtr4_nif
ms$ee16="Intel EtherExpress 16 or 16TP",301,ndis,ethernet,real,ms$ee16,ms$ee16_nif
ms$inteisa="Intel TokenExpress EISA 16/4",302,ndis,tokenring,real,ms$oli164,ms$oli164_nif
ms$intisa="Intel TokenExpress 16/4",303,ndis,tokenring,real,ms$oli164,ms$oli164_nif
ms$intmc="Intel TokenExpress MCA 16/4",304,ndis,tokenring,real,ms$oli164,ms$oli164_nif
ms$ntethnd="National Semiconductor Ethernode *16AT",351,ndis,ethernet,real,ms$ne2000,ms$ne2clone_nif
ms$ntat3="National Semiconductor AT/LANTIC EtherNODE 16-AT3",352,ndis,ethernet,real,ms$ne2000,ms$ne2clone_nif
ms$ncrtr4="NCR Token-Ring 4 Mbs ISA",362,ndis,tokenring,real,ms$ncrtr,ms$ncrtr4_nif
ms$ncrtr6="NCR Token-Ring 16/4 Mbs ISA",365,ndis,tokenring,real,ms$ncrtr,ms$ncrtr6_nif
ms$ncrtrmc="NCR Token-Ring 16/4 Mbs MCA",135,ndis,tokenring,real,ms$ncrtr,ms$ncrtrmc_nif
ms$ne1clone="NE1000 Compatible",213,ndis,ethernet,real,ms$ne1000,ms$ne1clone_nif
ms$ne2clone="NE2000 Compatible",214,ndis,ethernet,real,ms$ne2000,ms$ne2clone_nif
ms$ne1000="Novell/Anthem NE1000",211,ndis,ethernet,real,ms$ne1000,ms$ne1000_nif
ms$ne2000="Novell/Anthem NE2000",212,ndis,ethernet,real,ms$ne2000,ms$ne2000_nif
ms$ne1500="Novell/Anthem NE1500T",215,ndis,ethernet,real,ms$am2100,ms$am2100_nif
ms$ne2100="Novell/Anthem NE2100",216,ndis,ethernet,real,ms$am2100,ms$am2100_nif
ms$ne2="Novell/Anthem NE/2",103,ndis,ethernet,real,ms$ne2000,ms$ne2_nif
ms$oli164="Olicom 16/4 Token-Ring Adapter",401,ndis,tokenring,real,ms$oli164,ms$oli164_nif
ms$pro1340="Proteon ISA Token Ring (1340)",493,ndis,tokenring,real,ms$pro4,ms$pro4xt_nif,0x0002
ms$pro1342="Proteon ISA Token Ring (1342)",494,ndis,tokenring,real,ms$pro4,ms$pro4xt_nif,0x0002
ms$pro1346="Proteon ISA Token Ring (1346)",495,ndis,tokenring,real,ms$pro4,ms$pro4at_nif,0x0002
ms$pro1347="Proteon ISA Token Ring (1347)",496,ndis,tokenring,real,ms$pro4,ms$pro4at_nif,0x0002
ms$pro1840="Proteon MCA Token Ring (1840)",231,ndis,tokenring,real,ms$pro4,ms$pro4mc_nif,0x0002
ms$pro1390="Proteon Token Ring (P1390)",491,ndis,tokenring,real,ms$p139,ms$p139_nif
ms$pro1392="Proteon Token Ring (P1392)",492,ndis,tokenring,real,ms$p139,ms$p139_nif
ms$pdiarc8="Pure Data PDI508+ (ArcNet)",486,ndis,arcnet,real,ms$SMCARC,ms$pdi508_nif
ms$pdiarc16="Pure Data PDI516+ (ArcNet)",487,ndis,arcnet,real,ms$SMCARC,ms$pdi516_nif
ms$pditok32="Pure Data PDI9025-32 (Token Ring)",484,ndis,tokenring,real,ms$oli164,ms$oli164_nif
ms$pdutok="Pure Data PDuC9025 (Token Ring)",485,ndis,tokenring,real,ms$oli164,ms$oli164_nif
ms$ni6510="Racal NI6510",275,ndis,ethernet,real,ms$ni65,ms$ni65_nif
ms$rad="RadiSys EXM-10",541,ndis,ethernet,real,ms$WD80XX,ms$rad_nif
ms$smcpc="SMC ARCNETPC",221,ndis,arcnet,real,ms$SMCARC,ms$smcpc_nif
ms$smc100="SMC ARCNET PC100,PC200",222,ndis,arcnet,real,ms$SMCARC,ms$smcpc_nif
ms$smc110="SMC ARCNET PC110,PC210,PS110,PS210,PC250",223,ndis,arcnet,real,ms$SMCARC,ms$smcpc_nif
ms$smc130="SMC ARCNET PC130/E",224,ndis,arcnet,real,ms$SMCARC,ms$smc130_nif
ms$smc220="SMC ARCNET PC120,PC220,PC260",225,ndis,arcnet,real,ms$SMCARC,ms$smc220_nif
ms$smc270="SMC ARCNET PC270/E",226,ndis,arcnet,real,ms$SMCARC,ms$smc130_nif
ms$smc600="SMC ARCNET PC600W,PC650W",229,ndis,arcnet,real,ms$SMCARC,ms$smc600_nif
ms$gentcc="Thomas Conrad (All Types)",806,ndis,arcnet,real,ms$TC6X4X,ms$gentcc_nif
ms$tc6042e="Thomas Conrad TC6042",252,ndis,arcnet,real,ms$TC6X4X,ms$TC6X42_nif
ms$tc6045e="Thomas Conrad TC6045",251,ndis,arcnet,real,ms$TC6X4X,ms$TC6X45_nif
ms$tc6142e="Thomas Conrad TC6142",253,ndis,arcnet,real,ms$TC6X4X,ms$TC6X42_nif
ms$tc6145e="Thomas Conrad TC6145",254,ndis,arcnet,real,ms$TC6X4X,ms$TC6X45_nif
ms$tc6242e="Thomas Conrad TC6242",255,ndis,arcnet,real,ms$TC6X4X,ms$TC6X42_nif
ms$tc6245e="Thomas Conrad TC6245",256,ndis,arcnet,real,ms$TC6X4X,ms$TC6245_nif
ms$smc3k="SMC 3000 Series",551,ndis,ethernet,real,ms$smc3k,ms$smc3k_nif
ms$smcgen="SMC (WD) EtherCard (All Types except 8013/A)",803,ndis,ethernet,real,ms$WD80XX,ms$smcgen_nif
ms$w8003e="SMC (WD) EtherCard PLUS (WD/8003E)",293,ndis,ethernet,real,ms$WD80XX,ms$WD80XX_nif
ms$w8003wa="SMC (WD) EtherCard PLUS 10T/A (MCA) (WD 8003W/A)",112,ndis,ethernet,real,ms$WD80XX,ms$WD80XXa_nif
ms$w13ebt="SMC (WD) EtherCard PLUS 16 With Boot ROM Socket (WD/8013EBT)",298,ndis,ethernet,real,ms$WD80XX,ms$w8013ebt_nif
ms$w8003ea="SMC (WD) EtherCard PLUS/A (MCA) (WD 8003E/A or 8003ET/A)",110,ndis,ethernet,real,ms$WD80XX,ms$WD80XXa_nif
ms$w8003wt="SMC (WD) EtherCard PLUS TP (WD/8003WT)",296,ndis,ethernet,real,ms$WD80XX,ms$WD80XX_nif
ms$w8003eb="SMC (WD) EtherCard PLUS With Boot ROM Socket (WD/8003EB)",295,ndis,ethernet,real,ms$WD80XX,ms$WD80SS_nif
ms$w03ebt="SMC (WD) EtherCard PLUS With Boot ROM Socket (WD/8003EBT)",294,ndis,ethernet,real,ms$WD80XX,ms$WD80XX_nif
ms$w03ep="SMC (WD) EtherCard PLUS Elite (WD/8003EP)",451,ndis,ethernet,real,ms$WD80XX,ms$WD80SS_nif
ms$w03w="SMC (WD) EtherCard PLUS 10T (WD/8003W)",452,ndis,ethernet,real,ms$WD80XX,ms$WD80SS_nif
ms$w13ep="SMC (WD) EtherCard PLUS Elite 16 (WD/8013EP)",453,ndis,ethernet,real,ms$WD80XX,ms$WD80SS_nif
ms$w13w="SMC (WD) EtherCard PLUS Elite 16T (WD/8013W)",454,ndis,ethernet,real,ms$WD80XX,ms$WD80SS_nif
ms$w13ew="SMC (WD) EtherCard PLUS Elite 16 Combo (WD/8013EW or 8013EWC)",455,ndis,ethernet,real,ms$WD80XX,ms$WD80SS_nif
ms$w8003s="SMC (WD) StarCard PLUS (WD/8003S)",291,ndis,ethernet,real,ms$WD80XX,ms$WD80XX_nif
ms$w03sta="SMC (WD) StarCard PLUS/A (MCA) (WD 8003ST/A)",111,ndis,ethernet,real,ms$WD80XX,ms$WD80XXa_nif
ms$w8003sh="SMC (WD) StarCard PLUS With On Board Hub (WD/8003SH)",292,ndis,ethernet,real,ms$WD80XX,ms$WD80XX_nif
ms$xirc1="Xircom Pocket Ethernet I",532,ndis,ethernet,real,ms$xirc1,ms$xirc_nif
ms$xirc="Xircom Pocket Ethernet II",531,ndis,ethernet,real,ms$xirc,ms$xirc_nif
ms$znote="Zenith Data Systems Z-Note",521,ndis,ethernet,real,ms$znote,ms$znote_nif

[transport]
;   key=description,MSID, type, transport, mode, install, protini, winnet type, style
;       key:            unique identifier
;       description:    text description in quotes
;       MSID:           stack id (see trandefs.h)
;       type:           ndis|nonetbios
;       transport:      ipx|netbeui|tcp|xns
;       mode:           real|vxd
;       exclusive:      0 | 1
;       lanabse method: implicit | lanabase | drivername
;       install:        section name of install script
;       protini:        section name of protocol.ini script
;       winnet type:    net id
;       style:          0x0001  Not compatible with prot-mode netcards

ms$netbeui="Microsoft NetBEUI",1,ndis,netbeui,realvxd,0,lanabase,ms$netbeui,ms$netbeui_xif
ms$ipx="Novell IPX",101,nonetbios,ipx,real,1,implicit,ms$ipx,ms$ipx_xif,0x300
ms$ipx_tr="Novell IPX (Token Ring)",102,nonetbios,ipx,real,1,implicit,ms$ipx_tr,ms$ipx_tr_xif,0x300

;
; Install Sections
;
    ; install=section_name         // Install from a different section
    ; devdir=filelist              // copy files to the device dir
    ; netdir=filelist              // copy files to the network dir
    ; windir=filelist              // copy files to the windows dir
    ; sysdir=filelist              // copy files to the windows\system dir
    ; device=lookupname,commandline,after1,after2
    ;                              // add DEVICE=commandline to config.sys
    ; tsr=lookupname,commandline,after1,after2
    ;                              // add commandline to autoexec.bat before binding
    ; load=lookupname,commandline,after1,after2
    ;                              // add commandline to autoexec.bat after binding
    ; vxd=lookupname,commandline      // add a device= vxd to system.ini
    ; transport=lookupname,commandline// add a transport= vxd to system.ini
    ; netcard=lookupname,commandline  // add a netcard= vxd to system.ini
    ; secondnet=lookupname,commandline // add a secondnet= vxd to system.ini
    ;
    ;   lookupname: text used to search for the line in the file
    ;   commandline: text to add the line to the file (includes @path\ and params)
    ;   after1:     add line after line containing this text (optional)
    ;   after2:     secondary search if after1 not found

;
; Protocol Sections
;
    ; drivername=drivername                // drivername entry
    ; mem=key,,type,range,default,flags    // ram memory address
    ; io=key,,type,range,default,flags     // io base address
    ; irq=key,,type,range,default,flags    // irq setting
    ; param=key,description,type,range,default,flags  // other parameters

    ; types:      type      range               default
    ;             ----      -----               -------
    ;             static,   default,            n/a     // replace @netdir...
    ;             text,     "value,value,...",  default
    ;             chars,    numofchars,         default
    ;             keyonly   n/a                 n/a
    ;             int,      "first,last,step",  default
    ;             hex,      "first,last,step",  default
    ;
    ; flags:
    ; The flags field indicates special processing for the parameter
    ; Current flags are:
    ;   NWS_PARM_MEM_ABSOLUTE   0x00000001      memory address absolute (not paragraphs)
    ;   NWS_PARM_OPTIONAL       0x00000002      optional parameter
    ;   NWS_PARM_SOFTSET        0x00000004      software set parameter

; Protman Install and Protocol Sections

[protman_install]
descr="Microsoft Protocol Manager"
devdir=A:protman.dos,A:protman.exe
device=protman.dos,"@devdir\protman.dos /i:@devdir"
tsr=netbind
tsr="net start","@netdir\net start"

[protman]
drivername=PROTMAN$
param=PRIORITY,,static,MS$NETBEUI

;
; Netcard Install and Protocol Sections
;

; 3Com EtherLink MC

[ms$elnkmc]
devdir= A:elnkmc.dos
device=elnkmc.dos,@devdir\elnkmc.dos

[ms$elnkmc_nif]
drivername=ELNKMC$
param=MAXTRANSMITS,"Maximum Transmits",int,"8,50,1",12,0x02
slot=SLOTNUMBER,"Adapter Slot Number",int,"1,8,1",1,0x02

; Common IBM token ring install
;
; Cards that use this section:
;   ibmtra, ibmtr416a 
;   ibmtr1, ibmtr2, ibmtr2s, ibmtr416

[ms$IBMTOK]
devdir= A:ibmtok.dos
device=ibmtok.dos,@devdir\ibmtok.dos

; IBM Token Ring (ISA)

[ms$genibmtok_nif]
drivername=IBMTOK$
param=maxtransmits,"Maximum Transmits",int,"6,50,1",6,0x02
param=earlyrelease,"Early Release Option",keyonly,,,0x02
param=primary,"Primary Adapter",keyonly,,,0x02
param=alternate,"Alternate Adapter",keyonly,,,0x02
param=productid,"Product ID",chars,36,"0110F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=ram,"Physical RAM Location",hex,"0xA000,0xF000,0x200",0xD800, 0x02
param=recvbufs,"Receive Buffers",int,"2,60,1",2,0x02
param=recvbufsize,"Receive Buffer Size",int,"256,17952,8",256,0x02
param=xmitbufs,"Transmit Buffers",int,"1,2,1",1,0x02
param=xmitbufsize,"Transmit Buffer Size",int,"256,17952,8",256,0x02

[ms$ibmtr1_nif]
drivername=IBMTOK$
param=maxtransmits,"Maximum Transmits",int,"6,50,1",6,0x02
param=primary,"Primary Adapter",keyonly,,,0x02
param=alternate,"Alternate Adapter",keyonly,,,0x02
param=productid,"Product ID",chars,36,"0110F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=ram,"Physical RAM Location",hex,"0xA000,0xF000,0x800",0xD800, 0x02
param=recvbufs,"Receive Buffers",int,"2,60,1",2,0x02
param=recvbufsize,"Receive Buffer Size",int,"256,2040,8",256,0x02
param=xmitbufs,"Transmit Buffers",int,"1,2,1",1,0x02
param=xmitbufsize,"Transmit Buffer Size",int,"256,2040,8",2040,0x02

; IBM Token Ring II (ISA)

[ms$ibmtr2_nif]
drivername=IBMTOK$
param=maxtransmits,"Maximum Transmits",int,"6,50,1",6,0x02
param=primary,"Primary Adapter",keyonly,,,0x02
param=alternate,"Alternate Adapter",keyonly,,,0x02
param=productid,"Product ID",chars,36,"0110F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=ram,"Physical RAM Location",hex,"0xA000,0xF000,0x200",0xD800, 0x02
param=recvbufs,"Receive Buffers",int,"2,60,1",2,0x02
param=recvbufsize,"Receive Buffer Size",int,"256,2040,8",256,0x02
param=xmitbufs,"Transmit Buffers",int,"1,2,1",1,0x02
param=xmitbufsize,"Transmit Buffer Size",int,"256,2040,8",2040,0x02

; IBM TokenRing 4/16 

[ms$ibmtr4_nif]
drivername=IBMTOK$
param=earlyrelease,"Early Release Option",keyonly,,,0x02
param=maxtransmits,"Maximum Transmits",int,"6,50,1",6,0x02
param=primary,"Primary Adapter",keyonly,,,0x02
param=alternate,"Alternate Adapter",keyonly,,,0x02
param=productid,"Product ID",chars,36,"0110F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=recvbufs,"Receive Buffers",int,"2,60,1",2,0x02
param=recvbufsize,"Receive Buffer Size",int,"256,17952,8",256,0x02
param=xmitbufs,"Transmit Buffers",int,"1,2,1",1,0x02
param=xmitbufsize,"Transmit Buffer Size",int,"256,17952,8",256,0x02

; IBM TokenRing (MCA)

[ms$ibmtra_nif]
drivername=IBMTOK$
param=maxtransmits,"Maximum Transmit",int,"6,50,1",6,0x02
param=primary,"Primary Adapter",keyonly,,,0x02
param=alternate,"Alternate Adapter",keyonly,,,0x02
param=productid,"Product ID",chars,36,"0110F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=recvbufs,"Receive Buffers",int,"2,60,1",2,0x02
param=recvbufsize,"Receive Buffer Size",int,"256,2040,8",256,0x02
param=xmitbufs,"Transmit Buffers",int,"1,2,1",1,0x02
param=xmitbufsize,"Transmit Buffer Size",int,"256,2040,8",2040,0x02

; SMC 3000 Series

[ms$smc3k]
devdir= A:smc3000.dos
device=smc3000.dos,@devdir\smc3000.dos

[ms$smc3k_nif]
drivername=SMC_ETH$
irq=INTERRUPT,,text,"3,4,5,7,9,10",3
io=PORT_NUM,,hex,"0x200,0x3e0,0x20",0x300
param=MICRO_CHANNEL,"Force MCA Bus","0,1,1",0,0x02
param=XT_TYPE,"8 Bit Mode","0,1,1",0,0x02

; Generic install for SMC (WD) EtherCard PLUS series cards
;
;   WD8003EBT, WD8003SH, WD8003E, WD8003S, WD8003WT
;   WD8003EB, WD8003EP, WD8003W, WD8013EP, WD8013W, WD8013EW
;   WD8003ET/A, WD8003W/A, WD8003E/A, WD8003ST/A

[ms$WD80XX]
devdir= A:smcmac.dos
device=smcmac.dos,@devdir\smcmac.dos

[ms$smcgen_nif]
drivername=SMCMAC$
irq=irq,,int,"2,15,1",3
mem=ramaddress,,hex,"0xC000,0xEE00,0x0200",0xD000
io=iobase,,hex,"0x200,0x3e0,0x20",0x280
param=maxrequests,"Maximum Requests",int,"6,64,1",8,0x02
param=maxtransmits,"Maximum Transmits",int,"6,64,1",12,0x02
param=receivebuffers,"Receive Buffers",int,"6,96,1",12,0x02
param=receivebufsize,"Receive Buffer Size",int,"256,1536,1",256,0x02
param=receivechains,"Receive Chain Entries",int,"6,96,1",12,0x02

; This is the common _nif for the SCM (WD) 80xx series cards that are jumper set
;
;   WD8003EBT, WD8003SH, WD8003E, WD8003S, WD8003WT

[ms$WD80XX_nif]
drivername=SMCMAC$
irq=irq,,int,"2,7,1",3
mem=ramaddress,,hex,"0xC000,0xEE00,0x0200",0xD000
io=iobase,,hex,"0x200,0x3e0,0x20",0x280
param=maxrequests,"Maximum Requests",int,"6,64,1",8,0x02
param=maxtransmits,"Maximum Transmits",int,"6,64,1",12,0x02
param=receivebuffers,"Receive Buffers",int,"6,96,1",12,0x02
param=receivebufsize,"Receive Buffer Size",int,"256,1536,1",256,0x02
param=receivechains,"Receive Chain Entries",int,"6,96,1",12,0x02

; This is the common _nif for the WD 80xx series cards that ARE
; soft-settable
;
; Cards that use this section:
;   WD8003EB, WD8003EP, WD8003W, WD8013EP, WD8013W, WD8013EW

[ms$WD80SS_nif]
drivername=SMCMAC$
param=maxrequests,"Maximum Requests",int,"6,64,1",8,0x02
param=maxtransmits,"Maximum Transmits",int,"6,64,1",12,0x02
param=receivebuffers,"Receive Buffers",int,"6,96,1",12,0x02
param=receivebufsize,"Receive Buffer Size",int,"256,1536,1",256,0x02
param=receivechains,"Receive Chain Entries",int,"6,96,1",12,0x02

; This is the common _nif for the WD 80xx/A series cards
;
; Cards that use this section:
;
;   WD8003ET/A, WD8003W/A, WD8003E/A, WD8003ST/A

[ms$WD80XXa_nif]
drivername=SMCMAC$
slot=SlotNumber,"Adapter Slot Number",int,"1,8,1",1,0x02
param=maxrequests,"Maximum Requests",int,"6,64,1",8,0x02
param=maxtransmits,"Maximum Transmits",int,"6,64,1",12,0x02
param=receivebuffers,"Receive Buffers",int,"6,96,1",12,0x02
param=receivebufsize,"Receive Buffer Size",int,"256,1536,1",256,0x02
param=receivechains,"Receive Chain Entries",int,"6,96,1",12,0x02

[ms$rad_nif]
drivername=SMCMAC$
irq=irq,,int,"2,3,4,7",7
mem=ramaddress,,hex,"0xD000,0xDE00,0x0200",0xDE00
io=iobase,,hex,"0x200,0x3e0,0x20",0x240
param=maxrequests,"Maximum Requests",int,"6,64,1",8,0x02
param=maxtransmits,"Maximum Transmits",int,"6,64,1",12,0x02
param=receivebuffers,"Receive Buffers",int,"6,96,1",12,0x02
param=receivebufsize,"Receive Buffer Size",int,"256,1536,1",256,0x02
param=receivechains,"Receive Chain Entries",int,"6,96,1",12,0x02

; Novell/Anthem NE1000

[ms$ne1000]
devdir= A:ne1000.dos
device=ne1000.dos,@devdir\ne1000.dos

[ms$ne1000_nif]
drivername=MS1000$
io=IOBASE,,hex,"0x300,0x360,0x20",0x300
irq=INTERRUPT,,int,"2,5,1",3

[ms$ae1_nif]
drivername=MS1000$
io=IOBASE,,hex,"0x300,0x360,0x20",0x300
irq=INTERRUPT,,text,"2,3,4,5,6,7,10,15",15

[ms$ne1clone_nif]
drivername=MS1000$
io=IOBASE,,hex,"0x200,0x3E0,0x10",0x300
irq=INTERRUPT,,int,"2,15,1",3

; Novell/Anthem NE2000 and Clones

[ms$ne2000]
devdir= A:ne2000.dos
device=ne2000.dos,@devdir\ne2000.dos

[ms$ne2000_nif]
drivername=MS2000$
io=IOBASE,,hex,"0x300,0x360,0x20",0x300
irq=INTERRUPT,,int,"2,5,1",3

[ms$ae2_nif]
drivername=MS2000$
io=IOBASE,,hex,"0x300,0x360,0x20",0x300
irq=INTERRUPT,,text,"2,3,4,5,6,7,10,15",3

[ms$ne2_nif]
drivername=MS2000$

[ms$ae2mca_nif]
drivername=MS2000$
io=IOBASE,,text,"0x300,0x320,0x340,0x360,0x1000,0x2020,0x8020",0x1000
irq=INTERRUPT,,text,"3,4,5,9",3

[ms$ne2clone_nif]
drivername=MS2000$
io=IOBASE,,hex,"0x200,0x3E0,0x10",0x300
irq=INTERRUPT,,int,"2,15,1",3

; DEC EtherWorks Common Install

[ms$DEC_EW]
devdir= A:depca.dos
device=depca.dos,@devdir\depca.dos

[ms$decgen_nif]
drivername=DEPCA$
mem=RamAddress,,hex,"0xC000,0xE800,0x800",0xD000
irq=Interrupt,,text,"2,3,4,5,7,9,10,11,15",5
param=MaxMulticast,"Maximum Multicast Addresses",int,"1,256,1",8
param=MaxTransmits,"Maximum Transmits",int,"0,256,1",16
param=AdapterName,"Ethernet Adapter Name",text,"DEPCA,DE100,DE200,DE210","DE200",0x02

; DEC DEPCA

[ms$depca_nif]
drivername=DEPCA$
mem=RamAddress,,hex,"0xC000,0xE800,0x800",0xD000
irq=Interrupt,,text,"2,3,4,5,7",3
param=MaxMulticast,"Maximum Multicast Addresses",int,"1,256,1",8
param=MaxTransmits,"Maximum Transmits",int,"0,256,1",16
param=AdapterName,"Ethernet Adapter Name",static,"DEPCA",,0x02

; DEC EtherWorks LC  (DE10x Cards)

[ms$de100_nif]
drivername=DEPCA$
mem=RamAddress,,hex,"0xC000,0xE800,0x800",0xD000
irq=Interrupt,,text,"2,3,4,5,7",5
param=MaxMulticast,"Maximum Multicast Addresses",int,"1,256,1",8
param=MaxTransmits,"Maximum Transmits",int,"0,256,1",16
param=AdapterName,"Ethernet Adapter Name",static,"DE100",,0x02

; DEC EtherWorks Turbo (DE20x Cards)

[ms$de200_nif]
drivername=DEPCA$
mem=RamAddress,,hex,"0xC000,0xE800,0x800",0xD000
irq=Interrupt,,text,"5,9,10,11,15",5
param=MaxMulticast,"Maximum Multicast Addresses",int,"1,256,1",8
param=MaxTransmits,"Maximum Transmits",int,"0,256,1",16
param=AdapterName,"Ethernet Adapter Name",static,"DE200",,0x02

; DEC EtherWorks MCA Cards (DE21x Cards)

[ms$de210_nif]
drivername=DEPCA$
param=MaxMulticast,"Maximum Multicast Addresses",int,"1,256,1",8
param=MaxTransmits,"Maximum Transmits",int,"0,256,1",16
param=AdapterName,"Ethernet Adapter Name",static,"DE210",,0x02

; DECpc 433 Built-In Networking Card

[ms$decpc_nif]
drivername=DEPCA$
mem=RamAddress,,text,"0xD000",0xD000
irq=Interrupt,,text,"5",5
param=MaxMulticast,"Maximum Multicast Addresses",int,"1,256,1",8
param=MaxTransmits,"Maximum Transmits",int,"0,256,1",16
param=AdapterName,"Ethernet Adapter Name",static,"DE100",,0x02

; 3Com EtherLink Plus

[ms$elnkpl]
devdir= A:elnkpl.dos
device=elnkpl.dos,@devdir\elnkpl.dos

[ms$elnkpl_nif]
drivername=ELNKPL$
irq=INTERRUPT,,text,"3,4,5,6,7,9,10,11,12,14,15",3
io=IOADDRESS,,hex,"0x200,0x3f0,0x10",0x300
dma=DMACHANNEL,"DMA Channel",text,"1,3,5,6,7","1"

; 3Com EtherLink II

[ms$elnkii] 
devdir= A:elnkii.dos
device=elnkii.dos,@devdir\elnkii.dos

[ms$elnkii_nif] 
drivername=ELNKII$
irq=INTERRUPT,,int,"2,5,1",3
io=IOADDRESS,,text,"0x250,0x280,0x2A0,0x2E0,0x300,0x310,0x330,0x350",0x300
param=MAXTRANSMITS,"Maximum Transmits",int,"8,50,1",12
param=DATATRANSFER,"Data Transfer Mode",text,"block_dma,demand_dma,single_dma,pio_word,pio_byte",pio_word,0x02
dma=DMACHANNEL,"DMA Channel",int,"1,3,1",1,0x02
; NOTE: do not change the order of external and onboard.
; ncd_card_specific relies on this ordering.
param=TRANSCEIVER,"Transceiver Location",text,"external,onboard","onboard"
param=XMITBUFS,"Transmit Buffers",int,"1,2,1",2,0x02

; 3Com EtherLink III

[ms$elnk3]
devdir= A:elnk3.dos
device=elnk3.dos,@devdir\elnk3.dos

[ms$elnk3_nif]
DRIVERNAME = ELNK3$
io=IOADDRESS,,hex,"0x200,0x3F0,0x10",0x300
param=MAXTRANSMITS,"Maximum Transmits",int,"2,50,1",6
slot=SLOT,"Adapter Slot Number",int,"1,8,1",1,0x02

; 3Com TokenLink

[ms$toklnk]
devdir= A:tlnk.dos
device=tlnk.dos,@devdir\tlnk.dos

[ms$toklnk_nif]
drivername=TLNK$
irq=INTERRUPT,,text,"2,3,4,5,9,10,11,12,14",5
io=IOADDRESS,,text,"0x300,0x310,0x330,0x350","0x300"
dma=DMACHANNEL,"DMA Channel (0=None)",text,"0,1,3,5,6,7",0
param=MAXTRANSMITS,"Maximum Transmits",int,"8,40,1",8,0x02
param=PRODUCTID,"Product ID",chars,36,"0110F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=SPEED,"CPU Bus Speed",text,"6,8,10",6,0x02

; Thomas-Conrad TC6X4X Adapters

[ms$TC6X4X]
devdir= A:tccarc.dos
device=tccarc.dos,@devdir\tccarc.dos

[ms$gentcc_nif]
drivername=TCCARC$
irq=INTERRUPT,,text,"2,3,4,5,7,10,11,12,13,14,15",3
mem=MEMORYBASE,,hex,"0xC000,0xDC00,0x400",0xD000

[ms$TC6X42_nif]
drivername=TCCARC$
irq=INTERRUPT,,text,"2,3,4,5,7",3
mem=MEMORYBASE,,hex,"0xC000,0xDC00,0x400",0xD000

[ms$TC6X45_nif]
drivername=TCCARC$
irq=INTERRUPT,,text,"2,3,4,5,6,7,10,11,12,14,15",3
mem=MEMORYBASE,,hex,"0xC000,0xDC00,0x400",0xD000

[ms$TC6245_nif]
drivername=TCCARC$
irq=INTERRUPT,,text,"2,3,4,5,6,7,10,11,13,14,15",3
mem=MEMORYBASE,,hex,"0xC000,0xDC00,0x400",0xD000

; Common DCA 10 Mb install

[ms$DCA10]
devdir= A:mac586.sys
device=mac586.sys,@devdir\mac586.sys

; DCA 10 Mb ISA

[ms$DCA10_nif]
drivername=MAC586$
irq=INTERRUPT,,text,"2,3,4,5,7",3
mem=RAM,,text,"0xA000,0xA400,0xA800,0xAC00,0xC000,0xC400,0xCC00,0xD000,0xD400,0xD800,0xDC00","0xD800"
io=IOADDRESS,,text,"0x300,0x310,0x330,0x350","0x300"

; DCA 10 Mb MCA

[ms$DCA10mc_nif]
drivername=MAC586$
slot=SLOT,"Adapter Slot Number",int,"1,8,1",1,0x02

;R-I 6510

[ms$ni65]
devdir= A:ni6510.dos
device=ni6510.dos,@devdir\ni6510.dos

[ms$ni65_nif]
drivername=NI6510$
io=IOBASE,,hex,"0x300,0x360,0x20",0x360
param=MAXMULTICASTS,"Maximum Multicast Addresses",int,"1,16,1",10
param=MAXRECEIVES,"Maximum Receives",int,"1,8,1",4
param=MAXTRANSMITS,"Maximum Transmits",int,"1,50,1",6

;Cabletron E2000

[ms$cbl20xx]
devdir= A:e20ndis.dos
device=e20ndis.dos,@devdir\e20ndis.dos

[ms$cbl20xx_nif]
drivername=E20NDIS$
io=IOADDRESS,,text,"0x220,0x280,0x300,0x380",0x380
irq=INTERRUPT,,text,"3,4,5,6,7,9,10,11,12,14,15",3

;Cabletron E2100

[ms$cbl21xx]
devdir= A:e21ndis.dos
device=e21ndis.dos,@devdir\e21ndis.dos

[ms$cbl21xx_nif]
drivername=E21NDIS$
io=IOADDRESS,,text,"0x220,0x280,0x300,0x380",0x380
irq=INTERRUPT,,text,"3,4,5,6,7,9,10,11,12,14,15",3
mem=SHAREDRAM,,hex,"0xA000,0xEE00,0x200",0xD000
param=MEDIA,"Primary or Secondary Media",text,"PRI,SEC",PRI

; Western Digital 8013EBT

[ms$w8013ebt_nif]
drivername=SMCMAC$
irq=irq,,text,"2,3,4,5,7,10,11,15",3
mem=ramaddress,,hex,"0xC000,0xEE00,0x200",0xD000
io=iobase,,text,"0x200,0x220,0x240,0x260,0x280,0x2A0,0x2C0,0x300,0x340,0x380","0x280"
param=maxrequests,"Maximum Requests",int,"6,64,1",8,0x02
param=maxtransmits,"Maximum Transmits",int,"6,64,1",12,0x02
param=receivebuffers,"Receive Buffers",int,"6,96,1",12,0x02
param=receivebufsize,"Receive Buffer Size",int,"256,1536,1",256,0x02
param=receivechains,"Receive Chain Entries",int,"6,96,1",12,0x02

; Intel EtherExpress 16

[ms$ee16]
devdir= A:exp16.dos
device=exp16.dos,@devdir\exp16.dos

[ms$ee16_nif]
drivername=EXP16$
io=IOADDRESS,,text,"0x200,0x210,0x220,0x230,0x240,0x250,0x260,0x270,0x300,0x310,0x320,0x330,0x340,0x350,0x360,0x370","0x300",0x04
irq=IRQ,,text,"3,4,5,9,10,11",3,0x04
; NOTE: do not change the order or Early, Late, Never.
; ncd_card_specific relies on this ordering.
param=IOCHRDY,"I/O Channel Ready",text,"Early,Late,Never",Late,0x04
param=TRANSCEIVER,"Transceiver Type",text,"'Thick Net (AUI/DIX)','Thin Net (BNC/COAX)','Twisted-Pair (TPE)'","Thin Net (BNC/COAX)",0x04

; Olicom 16/4 Token-Ring Adapter ISA

[ms$oli164]
devdir= A:olitok.dos
device=olitok.dos,@devdir\olitok.dos

[ms$oli164_nif]
drivername=OLITOK$
param=adapter,"Adapter",int,"0,3,1",0,0x02
param=maxtransmits,"Maximum Transmits",int,"2,6,1",6
param=maxrequests,"Maximum General Requests",int,"1,10,1",6
param=recbufsize,"Receive Buffer Size",int,"256,5000,1",512
param=recbufcount,"Receive Buffers",int,"4,10,1",10
param=earlyrelease,"Early Token Release",text,"yes,no",yes
param=rpl,"RPL",keyonly,,,0x02

; 3Com EtherLink 16

[ms$elnk16]
devdir= A:elnk16.dos
device=elnk16.dos,@devdir\elnk16.dos

[ms$elnk16_nif]
drivername=ELNK16$

; SMC ARCNET Adapters

[ms$SMCARC]
devdir= A:SMC_ARC.DOS
device=SMC_ARC.DOS,@devdir\SMC_ARC.DOS

[ms$smcpc_nif]
drivername=SMC_ARC$
irq=interrupt,,text,"2,3,4,5,7","2"
io=iobase,,hex,"0x200,0x3F0,0x10",0x2E0
mem=memorybase,,hex,"0xC000,0xE000,0x1000",0xD000
param=micro_channel,"Force MCA Bus","0,1,1",0,0x02

[ms$smc130_nif]
drivername=SMC_ARC$
irq=interrupt,,text,"2,3,4,5,7","2"
io=iobase,,text,"0x260,0x290,0x2E0,0x2F0,0x300,0x350,0x380,0x3E0","0x2E0"
mem=memorybase,,text,"0xC000,0xC400,0xCC00,0xD000,0xD400,0xD800,0xDC00,0xE000",0xD000
param=micro_channel,"Force MCA Bus","0,1,1",0,0x02

[ms$smc220_nif]
drivername=SMC_ARC$
irq=interrupt,,text,"2,3,4,5,7","2"
io=iobase,,hex,"0x200,0x3F0,0x10",0x2E0
mem=memorybase,,hex,"0xC000,0xEC00,0x400",0xD000
param=micro_channel,"Force MCA Bus","0,1,1",0,0x02

[ms$smc600_nif]
drivername=SMC_ARC$
io=iobase,,text,"0x260,0x290,0x2E0,0x2F0,0x300,0x350,0x380,0x3E0","0x2E0"
irq=interrupt,,text,"2,3,4,5,7,9,10","2"
mem=memorybase,,text,"0xC000,0xC400,0xCC00,0xD000,0xD400,0xD800,0xDC00,0xE000",0xD000
param=micro_channel,"Force MCA Bus","0,1,1",0,0x02

[ms$genarc_nif]
drivername=SMC_ARC$
irq=interrupt,,int,"2,15,1","2"
io=iobase,,hex,"0x200,0x3F0,0x10",0x2E0
mem=memorybase,,hex,"0xC000,0xEC00,0x400",0xD000

[ms$pdi508_nif]
drivername=SMC_ARC$
irq=interrupt,,int,"2,7,1","2"
io=iobase,,text,"0x2A0,0x2E0,0x2F0,0x300",0x2E0
mem=memorybase,,text,"0xA000,0xC000,0xC400,0xCC00,0xD000,0xDC00,0xE000",0xD000

[ms$pdi516_nif]
drivername=SMC_ARC$
irq=interrupt,,text,"2,3,4,5,6,7,10","2"
io=iobase,,text,"0x220,0x240,0x250,0x2A0,0x2E0,0x2F0,0x300",0x2E0
mem=memorybase,,text,"0xC000,0xC400,0xCC00,0xD000,0xD400,0xDC00",0xD000

; Everex SpeedLink /PC16 (EV2027)

[ms$spdlk16]
devdir= A:evx16.dos
device=evx16.dos,@devdir\evx16.dos

[ms$spdlk16_nif]
drivername=EVX16$
irq=INTERRUPT,,text,"3,4,5,7,9,11,12,15",9
io=IOADDRESS,,text,"0x320,0x330,0x340,0x350,0x360,0x380,0x390,0x3A0","0x360"

; HP HPLANB Common Install (EtherNet Cards)

[ms$HPLANB]
devdir= A:hplanb.dos
device=hplanb.dos,@devdir\hplanb.dos

; HP PC LAN Adapters (Jumper Set: HP27245, HP27247A, HP27250)

[ms$hplanb_nif]
drivername=HPLANB$
irq=interrupt,,text,"3,4,5,7,9,10,11",3
io=ioaddress,,text,"0x200,0x240,0x280,0x2C0,0x300,0x320,0x340","0x300"
param=maxhwtrans,"Maximum Hardware Transmit Packets",int,"2,20,1",8
param=maxswtrans,"Maximum Software Transmit Packets",int,"1,20,1",2
param=maxmulticast,"Maximum Multicast Addresses",int,"1,200,1",5
param=maxicnest,"Max Nesting of Indication Completes",int,"1,4,1,",2

; NCR Token-Ring

[ms$ncrtr]
devdir= A:strn.dos
device=strn.dos,@devdir\strn.dos

[ms$ncrtr4_nif]
drivername=STRN$
param=TYPE,"Adapter Type",static,"TRISA4"
irq=INTERRUPT,,int,"2,7,1",2
io=PORT_ADDRESS,,text,"0x0A20,0x1A20",0x0A20
mem=SHARED_RAM,,text,"0xCA00,0xCC00,0xD000,0xD200,0xD400,0xD600",0xD000
param=PRODUCT_ID,"Product ID",chars,36,"0910F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=MAX_FRAME_SIZE,"Maximum Frame Size",int,"64,4472,1",2034
param=MAX_RECEIVES,"Maximum Receives",int,"2,50,1",3,0x02
param=RCV_BUF_SIZE,"Receive Buffer Size",int,"256,4472,1",2048,0x02
param=MAX_TRANSMITS,"Maximum Transmits",int,"2,50,1",6,0x02
param=MAX_REQUESTS,"Maximum Requests",int,"2,10,1",6,0x02

[ms$ncrtr6_nif]
drivername=STRN$
param=TYPE,"Adapter Type",static,"TRISA16"
param=BUS_MODE,"Bus Mode",static,"DIO"
irq=INTERRUPT,,text,"2,3,7,9,10,11,12,14,15",2
io=PORT_ADDRESS,,hex,"0x0A20,0x3A20,0x1000",0x0A20
dma=DMA_LEVEL,"DMA Channel",text,"3,5,6,7","5"
param=RING_SPEED,"Token Ring Speed (0=Use Card Settings)",text,"0,4,16",16
param=PRODUCT_ID,"Product ID",chars,36,"0910F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=MAX_FRAME_SIZE,"Maximum Frame Size",int,"64,17800,1",2034
param=MAX_RECEIVES,"Maximum Receives",int,"2,50,1",3,0x02
param=RCV_BUF_SIZE,"Receive Buffer Size",int,"256,17800,1",2048,0x02
param=MAX_TRANSMITS,"Maximum Transmits",int,"2,50,1",6,0x02
param=MAX_REQUESTS,"Maximum Requests",int,"2,10,1",6,0x02

[ms$ncrtrmc_nif]
drivername=STRN$
param=TYPE,"Adapter Type",static,"TRMC16"
param=PRODUCT_ID,"Product ID",chars,36,"0910F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0",0x02
param=MAX_FRAME_SIZE,"Maximum Frame Size",int,"64,17800,1",2034
param=MAX_RECEIVES,"Maximum Receives",int,"2,50,1",3,0x02
param=RCV_BUF_SIZE,"Receive Buffer Size",int,"256,17800,1",2048,0x02
param=MAX_TRANSMITS,"Maximum Transmits",int,"2,50,1",6,0x02
param=MAX_REQUESTS,"Maximum Requests",int,"2,10,1",6,0x02

[ms$p139]
devdir= A:NDIS39XR.DOS
devdir= A:PRORAPM.DWN
device=NDIS39XR.DOS,@devdir\NDIS39XR.DOS

[ms$p139_nif]
drivername=NDIS39XR$
irq=INTLEVEL,,text,"3,4,5,6,7,9,10,11,12",5
io=IOBASE,,hex,"0xA20,0xFE20,0x400",0xA20
dma=DMACHANNEL,"DMA Channel",text,"5,6,7,0",5
param=LINKSPEED,"Token Ring Speed",text,"4,16",16
param=MEDIA,"Cabling Type",text,"STP,UTP","STP"
param=DMACLOCK,"DMA Clock Speed",text,"4,8,BUS",8,0x02
param=SAEN,"Enable SAEN",text,"ON,OFF",ON,0x02
param=MAXTRANSMITS,"Maximum Transmits",int,"3,50,1",40,0x02

[ms$pro4]
devdir= A:PRO4.DOS
device=PRO4.DOS,@devdir\PRO4.DOS

[ms$pro4xt_nif]
drivername=PRO4$
irq=Interrupt,,int,"2,7,1",2
io=IOBASE,,hex,"0x100,0xFFF0,0x10",0xA20
mem=MEMBASE,,hex,"0xA000,0xFE00,0x200",0xE000

[ms$pro4at_nif]
drivername=PRO4$
irq=Interrupt,,text,"3,4,5,6,7,9,10,11,12",12
io=IOBASE,,hex,"0x100,0xFFF0,0x10",0xA20
dma=DMACHANNEL,"DMA Channel",text,"5,6,7",5

[ms$pro4mc_nif]
drivername=PRO4$
irq=Interrupt,,text,"3,4,5,7,10,11",3
io=IOBASE,,text,"0xA20,0x1A20,0x2A20,0x3A20,0x4A20,0x5A20,0xB20,0x1B20,0x2B20,0x3B20,0x4B20,0x5B20,0x820,0x1820,0x920,0x1920",0xA20

; Zenith Data Systems Z-Note

[ms$znote]
devdir= A:I82593.DOS
device=I82593.DOS,@devdir\I82593.DOS

[ms$znote_nif]
drivername=I82593$$
io=IOADDRESS,,static,"0x300"
irq=INTERRUPT,,static,"15"
param=DMACHAN0,"First DMA Channel",static,"6"
param=DMACHAN1,"Second DMA Channel",static,"7"
param=INBUFFER(K),"Receive Buffer",static,"8"
param=OUTBUFFERS(K),"Send Buffer",static,"3"

;Xircom Pocket Ethernet I

[ms$xirc1]
devdir= A:PENDIS.DOS
device=PENDIS.DOS,@devdir\PENDIS.DOS

;Xircom Pocket Ethernet II

[ms$xirc]
devdir= A:PE2NDIS.EXE
device=PE2NDIS.EXE,@devdir\PE2NDIS.EXE

[ms$xirc_nif]
DRIVERNAME=XIRCOM$

[ms$am2100]
devdir= A:am2100.dos
device=am2100.dos,@devdir\am2100.dos

[ms$am2100_nif]
DRIVERNAME=AM2100$
irq=INTERRUPT,,text,"3,4,5,9",9
io=IOADDRESS,,hex,"0x300,0x360,0x20",0x300
dma=DMACHANNEL,"DMA Channel",text,"3,5,6,7","5"

; Transport Install and Protocol Sections

[ms$netbeui]
sysdir=A:vnb.386
transport=vnb.386,vnb.386

[ms$netbeui_xif]
drivername=netbeui$
param=SESSIONS,"Maximum Sessions",int,"3,117,1",10
param=NCBS,"NCBS",int,"7,255,1",32

[ms$ipx]
;Standard IPX
devdir=A:msipx.sys
netdir=A:msipx.com
sysdir=A:vipx.386
secondnet=vipx.386,vipx.386
device=msipx.sys,@devdir\msipx.sys
load=msipx,@netdir\msipx,mscdex

[ms$ipx_tr]
;TokenRing IPX
install=ms$ipx
netdir=A:route.com
load=route,@netdir\route,msipx

[ms$ipx_xif]
DriverName=IPX$
; NOTE: do not change the order of Ethernet_II, Novell/Ethernet.
; ncd_trans_specific relies on this ordering.
param=MediaType,"Adapter Media Type",text,"Novell/Ethernet,'Ethernet_II (DIX)',","Novell/Ethernet"

[ms$ipx_tr_xif]
DriverName=IPX$
param=MediaType,"Adapter Media Type",static,"Token Ring",,

; Multi-Net

[MultiNet]
;key = description, net_type, exclusive,protocol id,install_section, style
lanman="Microsoft LAN Manager",0x200,0,0,mn$lanman
netware="Novell NetWare",0x0300,1,101,mn$netware

[mn$lanman]
sysdir=A:lmscript.exe
sysdir=A:lmscript.pif

[mn$netware]
install=delete_netware
netdir=A:netx.com
windir=A:nwpopup.exe
sysdir=A:vnetware.386,A:netware.drv,A:netware.hlp
secondnet.drv=netware.drv,netware.drv
secondnet=vnetware.386,vnetware.386
sysparm=NetWare,NWShareHandles,FALSE,noclobber
sysparm=NetWare,RestoreDrives,TRUE
sysparm=386Enh,OverlappedIO,off
winparm=windows,load,nwpopup.exe,append
load=netx,@netdir\netx,route,msipx
lastdrive=p

[delete_netware]
tsr=net3
tsr=net4
tsr=net5
tsr=emsnet3
tsr=emsnet4
tsr=emsnet5
tsr=emsnetx
tsr=xmsnet3
tsr=xmsnet4
tsr=xmsnet5
tsr=lsl
tsr=ipxodi
tsr=lansup
tsr=ipx
device=nwndis.dos
device=ipxndis.dos

[delete_drivers]
device=dxma0mod.sys
device=dxmc0mod.sys
device=dxmt0mod.sys
tsr=tokreui
tsr=netbios
