;***********************************************************************

;

; mwls97w8arm.inf

;

; Copyright (C) 2011, Marvell International Ltd.  

; All Rights Reserved

;

; Installation script for Marvell AVASTAR Family Wireless Network adapters.

;

;***********************************************************************



[Version]

 DriverVer=12/03/2012,14.62.17210.79

 Signature              = "$Windows NT$"

 Compatible             = 1

 Class                  = Net

 ClassGUID              = {4d36e972-e325-11ce-bfc1-08002be10318}

 Provider               = %MRVL_VER_VENDOR_NAME_STR%

 CatalogFile            = mwls97w8arm.cat

 PnpLockDown            = 1

[ControlFlags]

;Exclude all PNP adapters from user selection

 ExcludeFromSelect      = *



[Manufacturer]

 %MRVL_VER_VENDOR_NAME_STR% = mv14sd_models, NTarm



[mv14sd_models.NTarm]

 %MRVL_SD8797_DESC_STR% = mv14s6x.NTarm, SD\VID_02DF&PID_9129



;********************************************************************************

;					ARM Install section for Windows 8

;********************************************************************************

[mv14s6x.NTarm]

 Include=netvwifibus.inf

 Needs=VWiFiBus.CopyFiles

 AddReg                 = mv14s6x.reg, mv14s6x.sdio.reg, mv14s6x.common_ndis.reg, mv14x6x.params.reg, mv14x6x.WoWLANparams.reg, mv14x6x.Offloadparams.reg

 CopyFiles              = mv14s6x.copyfiles.NTarm

 Reboot
 
 ; BusType is not required in Win7, this is here just to satisfy ChkINF

 BusType                = 1

 Characteristics        = 0x84  ; NCF_PHYSICAL, NCF_HAS_UI

 *IfType                = 71    ; IF_TYPE_IEEE80211

 *MediaType             = 16    ; NdisMediumNative802_11

 *PhysicalMediaType     = 9     ; NdisPhysicalMediumNative802_11

 

[mv14s6x.NTarm.Services]

 Include=netvwifibus.inf

 Needs=VWiFiBus.Services

 AddService             = %MRVL_SDIO_SERVICE_STR%, 2, mv14s6x.Service.NTarm, mv14s6x.EventLog



[mv14s6x.Service.NTarm]

 DisplayName            = %MRVL_SDIO_SERVICE_STR%

 ServiceType            = 1     ; SERVICE_KERNEL_DRIVER

 StartType              = 3     ; SERVICE_DEMAND_START

 ErrorControl           = 1     ; SERVICE_ERROR_NORMAL

 ServiceBinary          = %12%\mwls97w8arm.sys

; LoadOrderGroup         = NDIS



[mv14s6x.NTarm.HW]

 Include=netvwifibus.inf

 Needs=VWiFiBus.PnPFilterRegistration



;********************************************************************************

;					Common Install section for Windows 8

;********************************************************************************

[mv14s6x.reg]

 HKR,NDI                ,DeviceID               ,0      ,"SD\VID_02DF&PID_9129"

 HKR,                   ,VendorDesc             ,0      ,%MRVL_SDIO_DESC_STR%

 HKR,                   ,NetworkAddress         ,0      ,""           



[mv14s6x.sdio.reg]

 HKR,NDI                ,Service                ,0      ,%MRVL_SDIO_SERVICE_STR%

 HKR,NDI                ,CardType               ,0      ,"SDIO"

 HKR,                   ,BusType                ,0      ,"0"

 

;*********************************************************************************************

[mv14s6x.EventLog]

 AddReg                 = mv14s6x.EventLog.reg



[mv14s6x.EventLog.reg]

 HKR,                   ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"

 HKR,                   ,TypesSupported         ,0x00010001     ,7



;*********************************************************************************************

[mv14s6x.common_ndis.reg]

HKR,                    ,DevLoader              ,0      ,"*ndis"

HKR,NDI                 ,Service                ,0      ,%MRVL_SDIO_SERVICE_STR%

HKR,NDI\Interfaces      ,UpperRange             ,0      ,"ndis5"

HKR,NDI\Interfaces      ,LowerRange             ,0      ,"ethernet,wlan,vwifi"

HKR,NDIS                ,LogDriverName          ,0      ,%MRVL_SDIO_SERVICE_STR%



[mv14x6x.params.reg]

;----------------------------------------------------------------------------

; RTS Threshold

;----------------------------------------------------------------------------

; HKR,NDI\Params\RTSThresh,ParamDesc             ,0      ,%RTSTHRESH_STR%

; HKR,NDI\Params\RTSThresh,Type                  ,0      ,int

; HKR,NDI\Params\RTSThresh,Default               ,0      ,2347

; HKR,NDI\Params\RTSThresh,Min                   ,0      ,256

; HKR,NDI\Params\RTSThresh,Max                   ,0      ,2347

HKR,,RTSThresh  ,0x00010001      ,2347


;----------------------------------------------------------------------------

; Fragmentation Threshold

;----------------------------------------------------------------------------

; HKR,NDI\Params\FragThresh,ParamDesc            ,0      ,%FRAGTHRESH_STR%

; HKR,NDI\Params\FragThresh,Type                 ,0      ,int

; HKR,NDI\Params\FragThresh,Default              ,0      ,2346

; HKR,NDI\Params\FragThresh,Min                  ,0      ,256

; HKR,NDI\Params\FragThresh,Max                  ,0      ,2346

; HKR,NDI\Params\FragThresh,Step                 ,0      ,2

HKR,,FragThresh  ,0x00010001      ,2346

;----------------------------------------------------------------------------

; Band to Use

;----------------------------------------------------------------------------

; HKR,NDI\Params\Band,ParamDesc                  ,0      ,%BAND_TO_USE_STR%

; HKR,NDI\Params\Band,Type                       ,0      ,enum

; HKR,NDI\Params\Band,Default                    ,0      ,"6"

; HKR,NDI\Params\Band\enum,"0"                   ,0      ,%1_INFRA_ABGN_STR%

; HKR,NDI\Params\Band\enum,"1"                   ,0      ,%2_INFRA_AN_STR%

; HKR,NDI\Params\Band\enum,"2"                   ,0      ,%3_INFRA_A_ONLY_STR%

; HKR,NDI\Params\Band\enum,"3"                   ,0      ,%4_INFRA_BGN_STR%

; HKR,NDI\Params\Band\enum,"4"                   ,0      ,%5_INFRA_BG_STR%

; HKR,NDI\Params\Band\enum,"5"                   ,0      ,%6_INFRA_B_ONLY_STR%

; HKR,NDI\Params\Band\enum,"6"                   ,0      ,%AUTO_STR%

HKR,,Band  ,0x00010001      ,6

;----------------------------------------------------------------------------

; Adhoc Band to Use

;----------------------------------------------------------------------------

; HKR,NDI\Params\AdhocBand,ParamDesc             ,0      ,%ADHOC_BAND_TO_USE_STR%

; HKR,NDI\Params\AdhocBand,Type                  ,0      ,enum

; HKR,NDI\Params\AdhocBand,Default               ,0      ,"0"

; HKR,NDI\Params\AdhocBand\enum,"0"              ,0      ,%1_ADHOC_BG_STR%

; HKR,NDI\Params\AdhocBand\enum,"1"              ,0      ,%2_ADHOC_BGN_STR%

; HKR,NDI\Params\AdhocBand\enum,"2"              ,0      ,%3_ADHOC_A_ONLY_STR%

; HKR,NDI\Params\AdhocBand\enum,"3"              ,0      ,%4_ADHOC_AN_STR%

HKR,,AdhocBand  ,0x00010001      ,0

;----------------------------------------------------------------------------

; Adhoc Channel

;----------------------------------------------------------------------------

; HKR,NDI\Params\AdhocChannel,ParamDesc          ,0      ,%ADHOC_CHANNEL_STR%

; HKR,NDI\Params\AdhocChannel,Type               ,0      ,enum

; HKR,NDI\Params\AdhocChannel,Default            ,0      ,"6"

; HKR,NDI\Params\AdhocChannel\enum,"1"           ,0      ,%BG_CHAN_01%

; HKR,NDI\Params\AdhocChannel\enum,"2"           ,0      ,%BG_CHAN_02%

; HKR,NDI\Params\AdhocChannel\enum,"3"           ,0      ,%BG_CHAN_03%

; HKR,NDI\Params\AdhocChannel\enum,"4"           ,0      ,%BG_CHAN_04%

; HKR,NDI\Params\AdhocChannel\enum,"5"           ,0      ,%BG_CHAN_05%

; HKR,NDI\Params\AdhocChannel\enum,"6"           ,0      ,%BG_CHAN_06%

; HKR,NDI\Params\AdhocChannel\enum,"7"           ,0      ,%BG_CHAN_07%

; HKR,NDI\Params\AdhocChannel\enum,"8"           ,0      ,%BG_CHAN_08%

; HKR,NDI\Params\AdhocChannel\enum,"9"           ,0      ,%BG_CHAN_09%

; HKR,NDI\Params\AdhocChannel\enum,"10"          ,0      ,%BG_CHAN_10%

; HKR,NDI\Params\AdhocChannel\enum,"11"          ,0      ,%BG_CHAN_11%

; HKR,NDI\Params\AdhocChannel\enum,"36"          ,0      ,%A_CHAN_36%

; HKR,NDI\Params\AdhocChannel\enum,"40"          ,0      ,%A_CHAN_40%

; HKR,NDI\Params\AdhocChannel\enum,"44"          ,0      ,%A_CHAN_44%

; HKR,NDI\Params\AdhocChannel\enum,"48"          ,0      ,%A_CHAN_48%

; HKR,NDI\Params\AdhocChannel\enum,"52"          ,0      ,%A_CHAN_52%

; HKR,NDI\Params\AdhocChannel\enum,"56"          ,0      ,%A_CHAN_56%

; HKR,NDI\Params\AdhocChannel\enum,"60"          ,0      ,%A_CHAN_60%

; HKR,NDI\Params\AdhocChannel\enum,"64"          ,0      ,%A_CHAN_64%

; HKR,NDI\Params\AdhocChannel\enum,"100"         ,0      ,%A_CHAN_100%

; HKR,NDI\Params\AdhocChannel\enum,"104"         ,0      ,%A_CHAN_104%

; HKR,NDI\Params\AdhocChannel\enum,"108"         ,0      ,%A_CHAN_108%

; HKR,NDI\Params\AdhocChannel\enum,"112"         ,0      ,%A_CHAN_112%

; HKR,NDI\Params\AdhocChannel\enum,"116"         ,0      ,%A_CHAN_116%

; HKR,NDI\Params\AdhocChannel\enum,"120"         ,0      ,%A_CHAN_120%

; HKR,NDI\Params\AdhocChannel\enum,"124"         ,0      ,%A_CHAN_124%

; HKR,NDI\Params\AdhocChannel\enum,"128"         ,0      ,%A_CHAN_128%

; HKR,NDI\Params\AdhocChannel\enum,"132"         ,0      ,%A_CHAN_132%

; HKR,NDI\Params\AdhocChannel\enum,"136"         ,0      ,%A_CHAN_136%

; HKR,NDI\Params\AdhocChannel\enum,"140"         ,0      ,%A_CHAN_140%

; HKR,NDI\Params\AdhocChannel\enum,"149"         ,0      ,%A_CHAN_149%

; HKR,NDI\Params\AdhocChannel\enum,"153"         ,0      ,%A_CHAN_153%

; HKR,NDI\Params\AdhocChannel\enum,"157"         ,0      ,%A_CHAN_157%

; HKR,NDI\Params\AdhocChannel\enum,"161"         ,0      ,%A_CHAN_161%

; HKR,NDI\Params\AdhocChannel\enum,"165"         ,0      ,%A_CHAN_165%

HKR,,AdhocChannel  ,0x00010001      ,6

;----------------------------------------------------------------------------

; Band Data Rate

;----------------------------------------------------------------------------

; HKR,NDI\Params\DataRate,ParamDesc              ,0      ,%BAND_DATARATE_STR%

; HKR,NDI\Params\DataRate,Type                   ,0      ,enum

; HKR,NDI\Params\DataRate,Default                ,0      ,"12"

; HKR,NDI\Params\DataRate\enum,"0"               ,0      ,%1_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"1"               ,0      ,%2_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"2"               ,0      ,%5_5_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"3"               ,0      ,%11_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"4"               ,0      ,%6_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"5"               ,0      ,%9_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"6"               ,0      ,%12_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"7"               ,0      ,%18_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"8"               ,0      ,%24_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"9"               ,0      ,%36_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"10"              ,0      ,%48_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"11"              ,0      ,%54_MBPS_STR%

; HKR,NDI\Params\DataRate\enum,"12"              ,0      ,%AUTO_STR%

 HKR,,DataRate  ,0x00010001      ,12

;----------------------------------------------------------------------------

; 11d Support

;----------------------------------------------------------------------------

; HKR,NDI\Params\EnableDot11d,ParamDesc          ,0      ,%ENABLE_DOT11D_STR%

; HKR,NDI\Params\EnableDot11d,Type               ,0      ,enum

; HKR,NDI\Params\EnableDot11d,Default            ,0      ,"1"

; HKR,NDI\Params\EnableDot11d\enum,"0"           ,0      ,%DISABLE_STR%

; HKR,NDI\Params\EnableDot11d\enum,"1"           ,0      ,%ENABLE_STR%

; HKR,NDI\Params\EnableDot11d,Optional           ,0      ,1

 HKR,,EnableDot11d  ,0x00010001      ,0

;----------------------------------------------------------------------------

; 11n Data Rate

;----------------------------------------------------------------------------

; HKR,NDI\Params\Dot11nDataRate,ParamDesc        ,0      ,%DOT11N_DATARATE_STR%

; HKR,NDI\Params\Dot11nDataRate,Type             ,0      ,enum

; HKR,NDI\Params\Dot11nDataRate,Default          ,0      ,"-1"

; HKR,NDI\Params\Dot11nDataRate\enum,"0"         ,0      ,%MCS0_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"1"         ,0      ,%MCS1_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"2"         ,0      ,%MCS2_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"3"         ,0      ,%MCS3_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"4"         ,0      ,%MCS4_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"5"         ,0      ,%MCS5_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"6"         ,0      ,%MCS6_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"7"         ,0      ,%MCS7_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"8"         ,0      ,%MCS8_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"9"         ,0      ,%MCS9_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"10"        ,0      ,%MCS10_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"11"        ,0      ,%MCS11_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"12"        ,0      ,%MCS12_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"13"        ,0      ,%MCS13_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"14"        ,0      ,%MCS14_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"15"        ,0      ,%MCS15_STR%

; HKR,NDI\Params\Dot11nDataRate\enum,"-1"        ,0      ,%AUTO_STR%

HKR,,Dot11nDataRate  ,0x00010001      ,-1

;----------------------------------------------------------------------------

; 11n Aggregation Mode options

;----------------------------------------------------------------------------

; HKR,NDI\Params\Dot11nAggMode,ParamDesc         ,0      ,%DOT11N_AGG_MODE_STR%

; HKR,NDI\Params\Dot11nAggMode,Type              ,0      ,enum

; HKR,NDI\Params\Dot11nAggMode,Default           ,0      ,"1"

; HKR,NDI\Params\Dot11nAggMode\enum,"0"          ,0      ,%DISABLED_STR%

; HKR,NDI\Params\Dot11nAggMode\enum,"1"          ,0      ,%AMPDU_STR%

HKR,,Dot11nAggMode  ,0x00010001      ,1

;----------------------------------------------------------------------------

; 11n Guard Interval

;----------------------------------------------------------------------------

; HKR,NDI\Params\GuardInterval,ParamDesc         ,0      ,%DOT11N_GI_STR%

; HKR,NDI\Params\GuardInterval,Type              ,0      ,enum

; HKR,NDI\Params\GuardInterval,Default           ,0      ,"0"

; HKR,NDI\Params\GuardInterval\enum,"0"          ,0      ,%LGI_STR%

; HKR,NDI\Params\GuardInterval\enum,"1"          ,0      ,%SGI_STR%

; HKR,NDI\Params\GuardInterval,Optional          ,0      ,1

HKR,,GuardInterval  ,0x00010001      ,0

;----------------------------------------------------------------------------

; Enable 11n Green Field

;----------------------------------------------------------------------------

; HKR,NDI\Params\EnableGF,ParamDesc              ,0      ,%DOT11N_GF_STR%

; HKR,NDI\Params\EnableGF,Type                   ,0      ,enum

; HKR,NDI\Params\EnableGF,Default                ,0      ,"0"

; HKR,NDI\Params\EnableGF\enum,"0"               ,0      ,%DISABLE_STR%

; HKR,NDI\Params\EnableGF\enum,"1"               ,0      ,%ENABLE_STR%

; HKR,NDI\Params\EnableGF,Optional               ,0      ,1

HKR,,EnableGF  ,0x00010001      ,0

;----------------------------------------------------------------------------

; Use 40MHz band

;----------------------------------------------------------------------------

; HKR,NDI\Params\AutoUse40MHz,ParamDesc          ,0      ,%DOT11N_USE_40MHZ_STR%

; HKR,NDI\Params\AutoUse40MHz,Type               ,0      ,enum

; HKR,NDI\Params\AutoUse40MHz,Default            ,0      ,"0"

; HKR,NDI\Params\AutoUse40MHz\enum,"0"           ,0      ,%NO_STR%

; HKR,NDI\Params\AutoUse40MHz\enum,"1"           ,0      ,%WHEN_POSSIBLE_STR%

; HKR,NDI\Params\AutoUse40MHz,Optional           ,0      ,1

HKR,,AutoUse40MHz,  0x00010001, 1

;----------------------------------------------------------------------------

; Enable Radio

;----------------------------------------------------------------------------

 HKR,,RadioEnabled                              ,0x00010001      ,1

 

;----------------------------------------------------------------------------

; Poor RSSI Factor

;----------------------------------------------------------------------------

 HKR,,PoorRssiFactor                            ,0x00010001      ,4



;----------------------------------------------------------------------------

; Roam BSS RSSI factor

;----------------------------------------------------------------------------

 HKR,,RoamBssRssiFactor                         ,0x00010001      ,3



;----------------------------------------------------------------------------

; ATIM Window size in TU

;----------------------------------------------------------------------------

 HKR,,ATIMWindow                                ,0x00010001      ,4



;----------------------------------------------------------------------------

; Sleep Period

;----------------------------------------------------------------------------

; HKR,NDI\Params\SleepPeriod,ParamDesc           ,0      ,%SLEEP_PERIOD_STR%

; HKR,NDI\Params\SleepPeriod,Type                ,0      ,int

; HKR,NDI\Params\SleepPeriod,Default             ,0      ,20

; HKR,NDI\Params\SleepPeriod,Min                 ,0      ,10

; HKR,NDI\Params\SleepPeriod,Max                 ,0      ,60

; HKR,NDI\Params\SleepPeriod,Optional            ,0      ,1

 HKR,,SleepPeriod,  0x00010001, 20

;----------------------------------------------------------------------------

; Inactivity Timeout

;----------------------------------------------------------------------------

; HKR,NDI\Params\InactivityTimeout,ParamDesc     ,0      ,%INACT_TIMEOUT_STR%

; HKR,NDI\Params\InactivityTimeout,Type          ,0      ,int

; HKR,NDI\Params\InactivityTimeout,Default       ,0      ,50

; HKR,NDI\Params\InactivityTimeout,Min           ,0      ,1

; HKR,NDI\Params\InactivityTimeout,Max           ,0      ,1000
 
 HKR,,InactivityTimeout,  0x00010001, 20


;----------------------------------------------------------------------------

; Local Listen Interval

;----------------------------------------------------------------------------

; HKR,NDI\Params\LocalListenInterval,ParamDesc   ,0      ,%LL_INTERVAL_STR%

; HKR,NDI\Params\LocalListenInterval,Type        ,0      ,int

; HKR,NDI\Params\LocalListenInterval,Default     ,0      ,0

; HKR,NDI\Params\LocalListenInterval,Min         ,0      ,0

; HKR,NDI\Params\LocalListenInterval,Max         ,0      ,20

 HKR,,LocalListenInterval,  0x00010001, 0


;----------------------------------------------------------------------------

; Power Save protocol options

;----------------------------------------------------------------------------

; HKR,NDI\Params\PSProto,ParamDesc                ,0      ,%PS_PROTO%

; HKR,NDI\Params\PSProto,Type                     ,0      ,enum

; HKR,NDI\Params\PSProto,Default                  ,0      ,"0"

; HKR,NDI\Params\PSProto\enum,"0"                 ,0      ,%IEEE_PS_STR%

; HKR,NDI\Params\PSProto\enum,"1"                 ,0      ,%PPS_PS_STR%

; HKR,NDI\Params\PSProto\enum,"2"                 ,0      ,%WMM_PS_STR%

; HKR,NDI\Params\PSProto\enum,"3"                 ,0      ,%UAPSD_PS_STR%

 HKR,,PSProto,  0x00010001, 0


;----------------------------------------------------------------------------

; Tx BF options

;----------------------------------------------------------------------------

; HKR,NDI\Params\BeamForming,ParamDesc           ,0      ,%BEAM_FORMING_STR%

; HKR,NDI\Params\BeamForming,Type                ,0      ,enum

; HKR,NDI\Params\BeamForming,Default             ,0      , "0"

; HKR,NDI\Params\BeamForming\enum,"0"            ,0      ,%DISABLED_STR%

; HKR,NDI\Params\BeamForming\enum,"1"            ,0      ,%ENABLE_STR%

HKR,,BeamForming,  0x00010001, 0


;----------------------------------------------------------------------------

; Number of Tx Buffers

;----------------------------------------------------------------------------

HKR,,NumOfTxBuffer                              ,0x00010001      ,256



;----------------------------------------------------------------------------

; Enable WPP tracing

;----------------------------------------------------------------------------

HKR,,EnableTracing                              ,0x00010001      ,1

 

;----------------------------------------------------------------------------

; Debug Mask for  Event Tracing or Debug prints 

; Default flags =(0x60400017) (MMSG |  MCMND| MFATAL | MERROR |MWARN | MINFO | MCMND | MOID)

;----------------------------------------------------------------------------

HKR,,DebugMask                                  ,0x00010001      ,0x68400037





;----------------------------------------------------------------------------

; Packet Coalescing Options

;----------------------------------------------------------------------------

 HKR,NDI\Params\*PacketCoalescing,ParamDesc      ,0      ,%PACKET_COALESCING%

 HKR,NDI\Params\*PacketCoalescing,Type           ,0      ,enum

 HKR,NDI\Params\*PacketCoalescing,Default        ,0      ,"1"

 HKR,NDI\Params\*PacketCoalescing\enum,"0"       ,0      ,%DISABLE_STR%

 HKR,NDI\Params\*PacketCoalescing\enum,"1"       ,0      ,%ENABLE_STR%




;----------------------------------------------------------------------------

; Enable WoWLan

;----------------------------------------------------------------------------

[mv14x6x.WoWLANparams.reg]

HKR,,EnableWOW                                  ,0x00010001      ,1

HKLM,"SYSTEM\CurrentControlSet\Services\NativeWifiP\Parameters",EnableWoWLAN,0x00010001,1

  

;----------------------------------------------------------------------------

; Wake On Pattern

;----------------------------------------------------------------------------

 HKR,NDI\Params\*WakeOnPattern,ParamDesc         ,0      ,%WakeOnPattern_STR%

 HKR,NDI\Params\*WakeOnPattern,Type              ,0      ,enum

 HKR,NDI\Params\*WakeOnPattern,Default           ,0      , "1"

 HKR,NDI\Params\*WakeOnPattern\enum,"0"          ,0      ,%DISABLED_STR%

 HKR,NDI\Params\*WakeOnPattern\enum,"1"          ,0      ,%ENABLED_STR%



;----------------------------------------------------------------------------

; Offload Parameters

;----------------------------------------------------------------------------

[mv14x6x.Offloadparams.reg]



;----------------------------------------------------------------------------

; ARP Offload

;----------------------------------------------------------------------------

 HKR,NDI\Params\*PMARPOffload,ParamDesc         ,0      ,%PMARPOffload_STR%

 HKR,NDI\Params\*PMARPOffload,Type              ,0      ,enum

 HKR,NDI\Params\*PMARPOffload,Default           ,0      , "1"

 HKR,NDI\Params\*PMARPOffload\enum,"0"          ,0      ,%DISABLED_STR%

 HKR,NDI\Params\*PMARPOffload\enum,"1"          ,0      ,%ENABLED_STR%

 

;----------------------------------------------------------------------------

; NS Offload

;----------------------------------------------------------------------------

 HKR,NDI\Params\*PMNSOffload,ParamDesc         ,0      ,%PMNSOffload_STR%

 HKR,NDI\Params\*PMNSOffload,Type              ,0      ,enum

 HKR,NDI\Params\*PMNSOffload,Default           ,0      , "1"

 HKR,NDI\Params\*PMNSOffload\enum,"0"          ,0      ,%DISABLED_STR%

 HKR,NDI\Params\*PMNSOffload\enum,"1"          ,0      ,%ENABLED_STR%

 

;----------------------------------------------------------------------------

; RSN Rekey Offload

;----------------------------------------------------------------------------

 HKR,NDI\Params\*PMWiFiRekeyOffload,ParamDesc  ,0      ,%PMWiFiRekeyOffload_STR%

 HKR,NDI\Params\*PMWiFiRekeyOffload,Type       ,0      ,enum

 HKR,NDI\Params\*PMWiFiRekeyOffload,Default    ,0      , "1"

 HKR,NDI\Params\*PMWiFiRekeyOffload\enum,"0"   ,0      ,%DISABLED_STR%

 HKR,NDI\Params\*PMWiFiRekeyOffload\enum,"1"   ,0      ,%ENABLED_STR%

 

 

;*********************************************************************************************

[DestinationDirs]

 DefaultDestDir               = 12 ; %windir%\system32\drivers

 

[SourceDisksNames]

 1 = %INSTALL_DISK_STR%



[SourceDisksFiles]

 mwls97w8arm.sys = 1

 

[mv14s6x.copyfiles.NTarm]

 mwls97w8arm.sys



;*********************************************************************************************

[Strings]

 MRVL_VER_VENDOR_STR          = "Marvell"

 MRVL_VER_VENDOR_NAME_STR     = "Marvell Semiconductor, Inc."

 MRVL_SD8797_DESC_STR         = "Marvell AVASTAR Wireless-N Network Controller (SDIO)"

 MRVL_SDIO_DESC_STR           = "Marvell AVASTAR Wireless-N Network Controller (SDIO)"

 MRVL_SDIO_SERVICE_STR        = "mwls97w8"

 INSTALL_DISK_STR             = "Marvell AVASTAR Wireless-N Software Install Disk"

 RTSTHRESH_STR                = "RTS Threshold"

 FRAGTHRESH_STR               = "Fragmentation Threshold"

 BAND_TO_USE_STR              = "Band to Use"

 ADHOC_BAND_TO_USE_STR        = "Adhoc Band to Use"

 ADHOC_CHANNEL_STR            = "Adhoc Channel"

 BAND_DATARATE_STR            = "11bg Transmit Data Rate"

 ENABLE_DOT11D_STR            = "11d Support"

 DOT11N_DATARATE_STR          = "11n Transmit Data Rate"

 DOT11N_AGG_MODE_STR          = "11n Aggregation Mode"

 DOT11N_GI_STR                = "11n Guard Interval"

 SGI_STR                      = "Short"

 LGI_STR                      = "Long"

 DOT11N_GF_STR                = "11n Green Field"

 DOT11N_RIFS_STR              = "11n Reduced IF Spacing"

 DOT11N_USE_40MHZ_STR         = "11n Use 40MHz Band"

 WHEN_POSSIBLE_STR            = "When Possible"

 BT_COEX                      = "Bluetooth Coex"

 PACKET_COALESCING            = "Packet Coalescing"

 SLEEP_PERIOD_STR             = "Sleep Interval"

 LL_INTERVAL_STR              = "Local Listen Interval"

 INACT_TIMEOUT_STR            = "Inactivity Timeout"

 ONBOARD_FW_STR               = "Enforce on board firmware"

 1_INFRA_ABGN_STR             = "1. 802.11abgn"

 2_INFRA_AN_STR               = "2. 802.11an"

 3_INFRA_A_ONLY_STR           = "3. 802.11a only"

 4_INFRA_BGN_STR              = "4. 802.11bgn"

 5_INFRA_BG_STR               = "5. 802.11bg"

 6_INFRA_B_ONLY_STR           = "6. 802.11b only"

 1_ADHOC_BG_STR               = "1. 802.11bg"

 2_ADHOC_BGN_STR              = "2. 802.11bgn"

 3_ADHOC_A_ONLY_STR           = "3. 802.11a only"

 4_ADHOC_AN_STR               = "4. 802.11an"

 1_MBPS_STR                   = "1. 1 Mbps"

 2_MBPS_STR                   = "2. 2 Mbps"

 5_5_MBPS_STR                 = "3. 5.5 Mbps"

 6_MBPS_STR                   = "4. 6 Mbps"

 9_MBPS_STR                   = "5. 9 Mbps"

 11_MBPS_STR                  = "6. 11 Mbps"

 12_MBPS_STR                  = "7. 12 Mbps"

 18_MBPS_STR                  = "8. 18 Mbps"

 24_MBPS_STR                  = "9. 24 Mbps"

 36_MBPS_STR                  = "10. 36 Mbps"

 48_MBPS_STR                  = "11. 48 Mbps"

 54_MBPS_STR                  = "12. 54 Mbps"

 AUTO_STR                     = "Auto"

 MCS0_STR                     = "MCS 0"

 MCS1_STR                     = "MCS 1"

 MCS2_STR                     = "MCS 2"

 MCS3_STR                     = "MCS 3"

 MCS4_STR                     = "MCS 4"

 MCS5_STR                     = "MCS 5"

 MCS6_STR                     = "MCS 6"

 MCS7_STR                     = "MCS 7"

 MCS8_STR                     = "MCS 8"

 MCS9_STR                     = "MCS 9"

 MCS10_STR                    = "MCS 10"

 MCS11_STR                    = "MCS 11"

 MCS12_STR                    = "MCS 12"

 MCS13_STR                    = "MCS 13"

 MCS14_STR                    = "MCS 14"

 MCS15_STR                    = "MCS 15"

 AMPDU_STR                    = "AMPDU"

 AMSDU_4K_STR                 = "AMSDU-4K"

 ENABLE_STR                   = "Enable"

 ENABLED_STR                  = "Enabled"

 DISABLE_STR                  = "Disable"

 DISABLED_STR                 = "Disabled"

 NO_STR                       = "No"

 YES_STR                      = "Yes"

 BG_CHAN_01                   = "1"

 BG_CHAN_02                   = "2"

 BG_CHAN_03                   = "3"

 BG_CHAN_04                   = "4"

 BG_CHAN_05                   = "5"

 BG_CHAN_06                   = "6"

 BG_CHAN_07                   = "7"

 BG_CHAN_08                   = "8"

 BG_CHAN_09                   = "9"

 BG_CHAN_10                   = "10"

 BG_CHAN_11                   = "11"

 A_CHAN_36                    = "36"

 A_CHAN_40                    = "40"

 A_CHAN_44                    = "44"

 A_CHAN_48                    = "48"

 A_CHAN_52                    = "52"

 A_CHAN_56                    = "56"

 A_CHAN_60                    = "60"

 A_CHAN_64                    = "64"

 A_CHAN_100                   = "100"

 A_CHAN_104                   = "104"

 A_CHAN_108                   = "108"

 A_CHAN_112                   = "112"

 A_CHAN_116                   = "116"

 A_CHAN_120                   = "120"

 A_CHAN_124                   = "124"

 A_CHAN_128                   = "128"

 A_CHAN_132                   = "132"

 A_CHAN_136                   = "136"

 A_CHAN_140                   = "140"

 A_CHAN_149                   = "149"

 A_CHAN_153                   = "153"

 A_CHAN_157                   = "157"

 A_CHAN_161                   = "161"

 A_CHAN_165                   = "165"

 PS_PROTO                     = "Power Save Protocol"

 WMM_PS_STR                   = "WMM PS"

 IEEE_PS_STR				  = "IEEE PS"

 PPS_PS_STR                   = "PPS"

 UAPSD_PS_STR                 = "uAPSD"

 BEAM_FORMING_STR             = "Beamformee"

 WakeOnMagicPacket_STR        = "Wake on magic packet"

 WakeOnPattern_STR            = "Wake on pattern match"  

 PMARPOffload_STR             = "ARP offload"

 PMNSOffload_STR              = "NS offload"

 PMWiFiRekeyOffload_STR       = "WiFi rekeying offload"

